Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package jain.protocol.ss7.oam.sccp

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the SCCP layer.

See:
Description

Interface Summary
ConcernedAreaMBean | This interface contains a list of remote Subsystems (SccpSaps) to be informed of local (primary broadcast) or remote (secondary broadcast) SCCP Subsystem status changes, or to be informed of the SCCP status after completion of SCCP Restart.
GlobalTitleEntryMBean | This class represents a Global Title entry (a combination of the global title translator and global title rule).
SccpEntitySetMBean | This class identifies the set of access points that result from a global title translation.
SccpLayerManagerMBean | This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
SccpManagedObjectMBean | This interface is used by an MBean to emit three differect types of Sccp Notifications.
SccpRoutingControlMBean | This interface defines the methods required by the SCCP Routing Control Function It defines methods to maintain management information concerning the SCCP routing control.
SccpSapMBean | This interface defines a SCCP Access Point (an SCCP Subsystem).
SccpTimerProfileMBean | This interface defines the specified timers for the SCCP Protocol Layer.

Class Summary
SccpAlarmNotification | A SccpAlarmNotification is an Notification emitted by a Sccp Managed Bean (MBean) to indicate a change in status of the MBean.
SccpErrorNotification | This Notification may be emitted by any Sccp Managed MBean if a user defined error is encountered.
SccpStatisticNotification | An SccpStatisticNotification is a Notification emitted by an SccpManagedObjectMBean containing the value of a particular statistic.

## Package jain.protocol.ss7.oam.sccp Description

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the SCCP layer. The diagram below shows the relationships between the SCCP Managed Beans.

- A Routing Control function (SccpRoutingControlMBean) shall control the SCCP routing for a single local signalling point (OwnSignallingPointMBean). Therefore, the SCCP Layer may have a number of RoutingControlMBeans, with each one having an association with a single local signalling point. Consequently, each Routing Control function (hence local signalling point) will have its own SccpTimerProfile.
- The SccpSapMBean represents any subsystem. On its own, the SccpSapMBean represents a remote subsystem, and is extended by LocalSubSystemMBean to represent a local subsystem. Each SccpSapMBean (subsystem) will have a single Mtp3SapMBean (signalling point) associated with it.
- Each routing control may therefore have a number of local (LocalSubSystemMBean) and remote (SccpSapMBean) subsystems associated with it.
- A GlobalTitleEntryMBean will translate to a single SccpEntitySetMBean. The SccpEntitySetMBean specifies how traffic is distributed between the two destination subsystems (SccpSapMBean).
- Each SccpSapMBean (subsystem) will have a single concerned area ConcernedAreaMBean) associated with it. The concerned area specifies all of a subsytem specifies the set of subsystems to be informed of subsystem status changes.

Relationship between the SCCP JAIN OAM MBeans

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems