Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

A B C D E G H I J L M N O P R S T

## A

addEntry(int, String, String) - Method in class jain.protocol.ss7.oam.CommitException
  Adds an entry to the log file of this CommitException.
addNotificationListenerToAllMBeans(NotificationListener, NotificationFilter, Object) - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Registers the specified NotificationListener with all of the OamManagedObjectMBeans of this Layer Manager.
ALARM_MO_ATTRIBUTE_VALUE_CHANGED - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Alarm Type Constant: Indicates that an attribute value changed.
ALARM_MO_CREATED - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Alarm Type Constant: Indicates that an instance of a Managed MBean has been created.
ALARM_MO_DELETED - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Alarm Type Constant: Indicates that an instance of a Managed MBean has been deleted.
ALARM_TIMER_EXPIRED - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Alarm Type Constant: Indicates that a timer has expired.
  IMPORTANT If an Alarm of this type is sent then the Timer Id of the Timer that caused this event should be set so that the application receiving the Notification can determine which Timer caused the Alarm.

## B

bytesToHex(byte[], int, int) - Static method in class jain.protocol.ss7.JainSS7Utility
  Convert an array of bytes to String with hex values.

## C

CATEGORY_CONFIGURATION - Static variable in class jain.protocol.ss7.oam.OamStatisticNotification
  A Statistic Category constant: Configuration management controls the resources of, and collects and provides data for, the signaling network and its components.
CATEGORY_FAULT - Static variable in class jain.protocol.ss7.oam.OamStatisticNotification
  A Statistic Category constant: Fault management encompasses fault detection, location, isolation and the correction of abnormal operation of the SS7 network.
CATEGORY_PERFORMANCE - Static variable in class jain.protocol.ss7.oam.OamStatisticNotification
  A Statistic Category constant: This enables the behavior of network resources and the effectiveness of communication activities in the network to be evaluated.
clearLinkSetList() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Removes all Linksets from this Linkset
commit() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Commit all operations on any Managed MBeans in this layer.
CommitException - exception jain.protocol.ss7.oam.CommitException.
  This Exception is thrown by a JAIN OAM Managed MBean if the commit() command has been invoked and not all of the operations were successfully comitted.
CommitException() - Constructor for class jain.protocol.ss7.oam.CommitException
  Constructs a new `CommitException`.
ConcernedAreaMBean - interface jain.protocol.ss7.oam.sccp.ConcernedAreaMBean.
  This interface contains a list of remote Subsystems (SccpSaps) to be informed of local (primary broadcast) or remote (secondary broadcast) SCCP Subsystem status changes, or to be informed of the SCCP status after completion of SCCP Restart.
CONG_CONGESTED_LEVEL1 - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
CONG_CONGESTED_LEVEL1 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Congestion Level constant: level 1
CONG_CONGESTED_LEVEL2 - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
CONG_CONGESTED_LEVEL2 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Congestion Level constant: level 2
CONG_CONGESTED_LEVEL3 - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
CONG_CONGESTED_LEVEL3 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Congestion Level constant: level 3
CONG_UNCONGESTED - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
CONG_UNCONGESTED - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Congestion Level constant: uncongested
createConcernedArea(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new Concerned Area Managed MBean containing the specified remote Subsystems (SccpSaps).
createGlobalTitleEntry(ObjectName, Integer, Byte[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new Global Title Entry Managed MBean.
createLink(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Link Managed Bean (LinkMBean).
createLinkSet(ObjectName, ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Linkset Managed Bean (LinkSetMBean).
createMtp2Sap(Integer) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Creates a new Mtp2SapMBean.
createMtp2TimerProfile() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Creates a new Mtp2 Timer Profile MBean that will use the correct Timer values for the the protocol variant of this Mtp2LayerManager.
createMtp3Sap(ObjectName, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Mtp3 Service Access Point MBean (representing a Remote Signalling Point)
createMtp3TimerProfile() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Mtp3TimerProfileMBean that will use the correct Timer values for the the protocol variant of this Mtp3LayerManager.
createOwnSignallingPoint(Long, Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Own Signalling Point Managed Bean (OwnSignallingPointMBean).
createRoute(ObjectName, ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Route Managed Bean (RouteMBean).
createRouteSet(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Routeset Managed Bean (RouteSetMBean).
createSccpEntitySet(ObjectName[], Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new SCCP Entity Set Managed MBean
createSccpRoutingControl(ObjectName, ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new Routing Control Managed MBean for the specified Own Signalling Point and (local) Subsystems
createSccpSap(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new SCCP Sevice Access Point (SAP) Managed MBean (a local or remote Subsystem)
createSccpTimerProfile() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Creates a new SccpTimerProfileMBean that will use the correct Timer values for the the protocol variant of this SccpLayerManager.
createScreeningTable() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Screening Table Managed Bean (ScreeningTableMBean).
createSignallingPoint(Long, Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Creates a new Own Signalling Point Managed Bean (OwnSignallingPointMBean).
createSS7Object(String) - Method in class jain.protocol.ss7.JainSS7Factory
  Returns an instance of a Peer JAIN SS7 Object identified by the supplied classname.
createTcapNode(ObjectName, ObjectName[]) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Creates a new TcapNodeMBean for the specified local signalling point and subsystem.

## D

deleteConcernedArea(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the Concerned Area Managed MBean identified by the specified ObjectName.
deleteGlobalTitleEntry(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the Global Title Entry Managed MBean identified by the specified ObjectName.
deleteLink(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the LinkMBean identified by the specified ObjectName.
deleteLinkSet(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the LinkSetMBean identified by the specified ObjectName.
deleteMtp2Sap(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Deletes the Mtp2SapMBean identified by the specified ObjectName.
deleteMtp2TimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Deletes the Mtp2TimerProfileMBean identified by the specified ObjectName.
deleteMtp3Sap(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the Mtp3SapMBean identified by the specified ObjectName.
deleteMtp3TimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the Mtp3TimerProfileMBean identified by the specified ObjectName.
deleteOwnSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the OwnSignallingPointMBean identified by the specified ObjectName.
deleteRoute(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the RouteMBean identified by the specified ObjectName.
deleteRouteSet(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the RouteSetMBean identified by the specified ObjectName.
deleteSccpEntitySet(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the SCCP Entity Set Managed MBean identified by the specified ObjectName.
deleteSccpRoutingControl(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the Routing Control Managed MBean identified by the specified ObjectName.
deleteSccpSap(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the SCCP Sevice Access Point (SAP) Managed MBean identified by the specified ObjectName (a local or remote Subsystem).
deleteSccpTimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Deletes the SccpTimerProfileMBean identified by the specified ObjectName.
deleteScreeningTable(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the ScreeningTableMBean identified by the specified ObjectName.
deleteSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Deletes the SignallingPointMBean identified by the specified ObjectName.
deleteTcapNode(ObjectName) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Deletes the specified TcapNodeMBean identified by the specified ObjectName Note that once a TcapNodeMBean has been deleted, it should no longer be returned by the getTcapNodes() method.
DISCARD_LEVEL_1 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Discard Level constant: level 1
DISCARD_LEVEL_2 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Discard Level constant: level 2
DISCARD_LEVEL_3 - Static variable in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  A Discard Level constant: level 3

## E

ES_EVEN - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Encoding Scheme constant:Encoding Scheme constants: Indicates a BCD, with an even number of digits.
ES_NATIONAL_SPECIFIC - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Encoding Scheme constant:Indicates National Specific encoding scheme for ITU.
ES_ODD - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Encoding Scheme constant:Indicates BCD, odd number of digits.
ES_UNKNOWN - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Encoding Scheme constant: Indicates an unknown encoding scheme.

## G

get(ObjectName) - Method in interface jain.protocol.ss7.oam.OamLookupTable
  Returns a reference to the object with the supplied ObjectName.
getActiveLinkCount() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns the number of links that should be active (alligned and ready for service) in this Linkset at all times.
getActiveMtp2Sap(Integer) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectName of one of the the Mtp2 Service Access Points (Mtp2SapMBeans) There is a subtle difference between this method and the getMtp2Saps() method in that this method returns the ObjectName of one of the Mtp2SapMBeans that are currently in use, whereas the getMtp2Saps() method returns the ObjectName of one of all the Mtp2SapMBeans (both those Mtp2SapMBeans currently in use and the Mtp2SapMBeans that have been configured are not available for use for any reason including for backup).
getActiveMtp2Saps() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectNames of all of the the Mtp2 Service Access Point MBeans (Mtp2SapMBeans).
getActiveOwnSignallingPoint(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the active (local) OwnSignallingPointMBeans of this stack.
  The underlying stack management system may support multiple signalling points on the the same system.
getActiveOwnSignallingPoints() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all of the active (local) OwnSignallingPointMBeans of this stack.
  The underlying stack management system may support multiple signalling points on the the same system.
getActiveSccpRoutingControl(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of the Active SCCP Routing controls of this SCCP Layer Manager.
getActiveSccpRoutingControls() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectNames of all the Active SCCP Routing controls of this SCCP Layer Manager.
getActiveTcapNode(Integer) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Returns the ObjectName of one of the active TCAP layers managed by this TCAP Layer Manager.
getActiveTcapNodes() - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Returns an array of ObjectNames of all the active TCAP layers managed by this TCAP Layer Manager.
getAddressInformation() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Gets the Address Information of this Global Title Entry.
getAdjacentSignallingPoint() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Gets the ObjectName of the Adjacent OwnSignallingPointMBean of this Linkset.
getAlarmType() - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Returns the Type of this Alarm
getAllOamManagedObjects() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Returns an array containing the ObjectNames all of the OamManagedObjectMBeans managed by this Layer Manager.
getAvailability() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Returns the availability of this Route [ITU Rec.
getBackup() - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Gets the ObjectName of the Backup OwnSignallingPointMBean of this OwnSignallingPointMBean.
getCategory() - Method in class jain.protocol.ss7.oam.OamStatisticNotification
  Returns the category of this OamStatisticNotification.
getCombinedLinkSet(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns the ObjectName of the LinkSet at the specified position in the array of the LinkSetMBeans with which this Linkset is combined.
getCombinedLinkSets() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns an array of ObjectNames of the LinkSetMBeans with which this Linkset is combined.
getConcernedArea() - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Returns the ObjectName of the concerned area to be used by SCCP Management for broadcasting the SCCP status after completion of SCCP Restart.
getConcernedArea(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the Concerned Areas created by this layer manager
getConcernedAreas() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectName of all Concerned Area MBeans created by this layer manager
getCongestionAbate(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the value at which a link congestion situation ends for the specified congestion level.
getCongestionLevel() - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Gets the Congestion Level of this Routeset.
getCongestionLevel() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Gets the Congestion Level of this Link.
getCongestionOnset(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the value at which a link congestion situation starts for the specified congestion level.
getCurrentCapacity() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the Current Capacity of this Link.
getCurrentCapacity() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns the Current Capacity of this Linkset.
getCurrentVal() - Method in interface jain.protocol.ss7.oam.OamTimerValMBean
  This method gets the current value for this timer in milliseconds.
getDestinationSubsystem(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Returns the ObjectName of one the destination Subsystems (SCCP SAPs) of this Entity Set.
getDestinationSubsystems() - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Returns the ObjectName of the destination Subsystems (SCCP SAPs) of this Entity Set.
getDestSignallingPoint() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Gets the ObjectName of the Signalling point (SignallingPointMBean) that identifies the Destination SignallingPointMBean of this RouteSetMBean.
getDiscardAbate(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the value at which MSUs are no longer discarded for the specified discard level.
getDiscardOnset(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the value at which MSUs are discarded for the specified discard level.
getEncodingScheme() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Gets the Encoding Scheme of this Global Title Entry.
getErrorType() - Method in class jain.protocol.ss7.oam.OamErrorNotification
  Returns the Type of this Error.
getFirstLinkSet() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Gets the ObjectName of the Linkset which is intended to be used as first segment of the succession of Linksets in this Route, which form the signalling route on the network level.
getGlobalTitleEntries() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectNames of all Global Tiltle Entries created by this layer manager
getGlobalTitleEntries() - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns an array of the ObjectNames of all Global Titles of this SCCP.
getGlobalTitleEntry(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the Global Tiltle Entries created by this layer manager
getGlobalTitleEntry(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns the ObjectName of the specified Global Title entry of this SCCP.
getGTIndicator() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Returns the Global Title indicator.
getInstance() - Static method in class jain.protocol.ss7.JainSS7Factory
  Returns an instance of a JainSS7Factory.
getJainObjectList() - Method in class jain.protocol.ss7.JainSS7Factory
  Returns a Vector containing all of the Peer JAIN Objects that have previously been created using this `JainSS7Factory`.
getLink(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the LinkMBeans created by this layer manager
getLink(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Gets the ObjectName of the signalling link at the specified position in the set of links of this linkset
getLinkCount() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Gets the Number of this Linkset.
getLinks() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the LinkMBeans created by this layer manager
getLinks() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Gets the ObjectNames of the list of signalling linkMBeans of this linkSetMBean
getLinkSet(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the LinkSetMBeans created by this layer manager
getLinkSet(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Gets the ObjectName of the Linkset at the specified position in the set of Linksets in this route
getLinkSets() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the LinkSetMBeans created by this layer manager
getLinkSets() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Gets an array of ObjectNames of the list of Linksets in this route
getLog() - Method in class jain.protocol.ss7.oam.CommitException
  Returns a log of the operations.
getLookupTable() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Returns a reference to the OamLookupTable.
getMaxCapacity() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the Maximum Capacity of this Link.
getMaxCapacity() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns the Maximum Capacity of this Linkset.
getMaxVal() - Method in interface jain.protocol.ss7.oam.OamTimerValMBean
  This method gets the maximum value for this timer in milliseconds.
getMinVal() - Method in interface jain.protocol.ss7.oam.OamTimerValMBean
  This method gets the minimum value for this timer in milliseconds.
getMtp2Sap() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the ObjectName of the Mtp2 Service Access Point MBean (Mtp2SapMBean) associated with this Signalling Link (LinkMBean).
getMtp2Sap(Integer) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectName of one of the Mtp2SapMBeans created by this layer manager
getMtp2Saps() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectNames of all of the Mtp2SapMBeans created by this layer manager
getMtp2TimerProfile() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  Returns the ObjectName of the MTP2 Timer Profile MBean containing the MTP2 Timer values to be used with this link.
getMtp2TimerProfile(Integer) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectName of one of the Mtp2TimerProfileMBeans created by this layer manager
getMtp2TimerProfiles() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Returns the ObjectNames of all of the Mtp2TimerProfileMBeans created by this layer manager
getMtp2TimerT1() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Alignment ready [ITU & ANSI].
getMtp2TimerT2() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Not aligned [ITU & ANSI].
getMtp2TimerT3() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Aligned [ITU & ANSI].
getMtp2TimerT4E() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Emergency proving period [ITU & ANSI].
getMtp2TimerT4N() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Normal proving period [ITU & ANSI].
getMtp2TimerT5() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Sending SIB [ITU & ANSI].
getMtp2TimerT6() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Remote congestion [ITU & ANSI].
getMtp2TimerT7() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean
  Returns the ObjectName of the Timer: Excessive delay of acknowledgement [ITU & ANSI].
getMtp3Sap() - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Returns the ObjectName of the MTP3 Access Point representing the Signalling Point (MTP) used by this SCCP.
getMtp3Sap(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the Mtp3SapMBeans (Remote Signalling Points) created by this layer manager
getMtp3Sap(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Returns an Mtp3Sap using this signalling point
getMtp3Saps() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the Mtp3SapMBeans (Remote Signalling Points) created by this layer manager
getMtp3Saps() - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Returns Mtp3Saps using this signalling point
getMtp3SapUser(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Gets an ObjectName of a particular user of this SAP
getMtp3SapUsers() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Gets an array of ObjectNames of the users of this SAP
getMtp3TimerProfile() - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Returns the ObjectName of the Mtp3TimerProfileMBean containing the MTP3 Timer values to be used with this OwnSignallingPointMBean
getMtp3TimerProfile(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the Mtp3TimerProfileMBeans created by this layer manager
getMtp3TimerProfiles() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the Mtp3TimerProfilesMBeans created by this layer manager
getMtp3TimerT1() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Delay to avoid message mis-sequencing on changeover [ITU & ANSI].
getMtp3TimerT10() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting to repeat signalling routeset test message [ITU & ANSI].
getMtp3TimerT11() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Transfer restricted timer [ITU & ANSI].
getMtp3TimerT12() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for uninhibit acknowledgement [ITU & ANSI].
getMtp3TimerT13() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for force uninhibit [ITU & ANSI].
getMtp3TimerT14() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Waiting for inhibition acknowledgement [ITU & ANSI].
getMtp3TimerT15() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting to start signalling routeset congestion test [ITU & ANSI].
getMtp3TimerT16() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for routeset congestion status update [ITU & ANSI].
getMtp3TimerT17() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Delay to avoid oscillation of initial alignment failure and link restart [ITU & ANSI].
getMtp3TimerT18() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer within a signalling point whose MTP restarts for supervising link and link set activation as well as the receipt of routing information [ITU].
  Not Used [ANSI].
getMtp3TimerT19() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Supervision timer during MTP restart to avoid possible ping-pong of TFP, TFR1 and TRA messages [ITU].
  Failed link craft referral timer [ANSI].
getMtp3TimerT2() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for changeover acknowledgement [ITU & ANSI].
getMtp3TimerT20() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Overall MTP restart timer at the signalling point whose MTP restarts [ITU].
  Waiting to repeat local inhibit test [ANSI].
getMtp3TimerT21() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Overall MTP restart timer at a signalling point adjacent to one whose MTP restarts [ITU].
  Waiting to repeat remote inhibit test [ANSI].
getMtp3TimerT22() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Local inhibit test timer [ITU].
  Timer at starting SP, waiting for signalling links to become available [ANSI].
getMtp3TimerT23() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Remote inhibit test timer [ITU].
  Timer at restating SP, started after Mtp3Timer22, waiting to receive all traffic restart allowed messages [ANSI].
getMtp3TimerT24() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Stabilising timer after removal of local processor outage, used in LPO latching to RPO (national option) [ITU].
getMtp3TimerT25() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer at SP adjacent to restarting SP, waiting for traffic restart allowed message [ANSI].
getMtp3TimerT26() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer at restarting SP, waiting to repeat traffic restart waiting message [ANSI].
getMtp3TimerT27() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Minimum duration of unavailability for full restart [ANSI].
getMtp3TimerT28() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer at SP adjacent to restarting SP, waiting for traffic restart waiting message [ANSI].
getMtp3TimerT29() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer started when TRA sent in response to unexpected TRA or TRW [ANSI].
getMtp3TimerT3() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Time controlled diversion-delay to avoid mis-sequencing on changeback [ITU & ANSI].
getMtp3TimerT30() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Timer to limit sending of TFPs and TFRs in response to unexpected TRA or TRW [ANSI].
getMtp3TimerT4() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for changeback acknowledgement (first attempt) [ITU & ANSI].
getMtp3TimerT5() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for changeback acknowledgement (second attempt) [ITU & ANSI].
getMtp3TimerT6() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Delay to avoid message mis-sequencing on controlled rerouting [ITU & ANSI].
getMtp3TimerT7() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Waiting for signalling data link connection acknowledgement [ITU & ANSI].
getMtp3TimerT8() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean
  Returns the ObjectName of the Timer: Transfer prohibited inhibition timer (transient solution) [ITU & ANSI].
getName() - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Gets the name of this OamManagedBean.
getNatureOfAddrInd() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Gets the Nature of Address Indicator of this Global Title Entry.
getNetworkIndicator() - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Gets the Network Indicator of this Signalling Point (one of the Network Indicator constants).
getNonOamErrorMsg() - Method in class jain.protocol.ss7.oam.OamErrorNotification
  Returns a non-OAM related error message.
getNumberingPlan() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Gets the Numbering Plan of this Global Title Entry.
getObjectId() - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Returns an object id that is unique within all objects of the same class.
getObjectName() - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Gets the ObjectName of this OamManagedObjectBean.
getObjectType() - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Returns the Object Type of this Managed Bean (MBean) as a String.
getObjectType() - Method in class jain.protocol.ss7.oam.TooManyInstancesException
  Returns an Type that identifies the Managed MBean type of which there are too many instances
getOwnSignallingPoint() - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns the ObjectName of the local Signalling Point governed by this routing control.
getOwnSignallingPoint() - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Returns the ObjectName of the signalling point of this TCAP Node
getOwnSignallingPoint(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of one of the OwnSignallingPointMBeans created by this layer manager
getOwnSignallingPoints() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the OwnSignallingPointMBeans created by this layer manager
getPathName() - Method in class jain.protocol.ss7.JainSS7Factory
  Returns the current Pathname.
getPortType() - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  Returns the clocking type of this port (DTE or DCE).
getPriority() - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Returns the Priority of this OamAlarmNotification.
getPriority() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Returns the priority of this Route within the containing Routeset.
getProprietaryInformation() - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Returns an Object that may contain proprietary methods for this Managed Bean (MBean).
getProtocolVariantAndYear() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Returns the Protocol variant and year.
getRemoteSubsystem(Integer) - Method in interface jain.protocol.ss7.oam.sccp.ConcernedAreaMBean
  Returns an ObjectName of the remote Subsystem from the list of Subsystems to be informed of local or remote subsystem status changes .
getRemoteSubsystems() - Method in interface jain.protocol.ss7.oam.sccp.ConcernedAreaMBean
  Returns an array of ObjectNames of the all the Subsystems to be informed of local or remote subsystem status changes
getRoute(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the RouteMBeans created by this layer manager
getRoute(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Gets the ObjectName of the RouteMBean at the specified position in this RouteSet.
getRoutes() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all of the RouteMBeans created by this layer manager
getRoutes() - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Returns the ObjectNames RouteMBeans in this routeset
getRouteSet(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the RouteSetMBeans created by this layer manager
getRouteSet(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Returns the ObjectName of the RouteSetMBean at the specified position in all of the RouteSetMBeans associated with this OwnSignallingPointMBean.
getRouteSets() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the RouteSetMBeans created by this layer manager
getRouteSets() - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Returns an array of ObjectNames of all the RouteSetMBeans associated with this OwnSignallingPointMBean.
getSapAvailabilityStatus() - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Returns the availability status of this SCCP (one of the SCCP SAP Status constants).
getSapStatus() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Returns the status of the signalling point identified by this Service Access Point (one of the SAP Status constants).
getSccpEntitySet() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Returns the ObjectName of the Entity Set of this GlobalTitle Entry.
getSccpEntitySet(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the SCCP Entity Sets created by this layer manager
getSccpEntitySets() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectName of all SCCP Entity Sets created by this layer manager
getSccpRoutingControl(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the SCCP Routing Controls created by this layer manager
getSccpRoutingControls() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectName of all SCCP Routing Controls created by this layer manager
getSccpSap(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the SCCP SAPs (Local or Remote Subsystems) created by this layer manager
getSccpSaps() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectNames of all SCCP SAPs (Local or Remote Subsystems) created by this layer manager
getSccpTimerConnect() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer Connect - Waiting for connection confirm message [ITU & ANSI].
getSccpTimerCoordChg() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Out-of-service Grant Timer - Waiting for grant for subsystem to go out-of-service.
getSccpTimerGuard() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer Guard - Waiting to resume normal procedure for temporary connection sections during the restart procedure [ITU & ANSI].
getSccpTimerIAR() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer IAR - Waiting to receive a message on a connection section [ITU & ANSI].
getSccpTimerIAS() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer IAS - Delay to send a message on a conn IT on a connection section when there are no messages to send [ITU & ANSI].
getSccpTimerIgnoreSST() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Ignore SST Timer - Delay for subsystem between receiving grant to go out-of-service and actually going out of service [ANSI].
getSccpTimerInt() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer Int - Waiting for release complete message; or to release connection resources, freeze the LRN and alert a maintenance function after the initial expiry [ITU].
getSccpTimerProfile() - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns the ObjectName of the SCCP Timer Profile MBean containing the SCCP Timer values
getSccpTimerProfile(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns the ObjectName of one of the SCCP Timer Profiles created by this layer manager
getSccpTimerProfiles() - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Returns an array of the ObjectNames of all SCCP Timer Profiles created by this layer manager
getSccpTimerReassembly() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Reassembly Timer - Waiting to receive all the segments of the remaining segments single segmented message after receiving the first segment [ITU].
getSccpTimerRelease() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer Release - Waiting for release complete message [ITU & ANSI].
getSccpTimerRepeatRelease() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Timer Repeat Release - Waiting for release complete message; or to repeat sending released message after the initial expiry [ITU].
getSccpTimerReset() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Reset Timer - Waiting to release temporary connection section or alert maintenance function after reset request message is sent [ITU & ANSI].
getSccpTimerRtgStatInfo() - Method in interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean
  Returns the ObjectName of the Timer: Routing Stat Info Timer - Delay between requests for subsystem routing status information [ANSI].
getScreeningTable(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectName of one of the ScreeningTableMBeans created by this layer manager
getScreeningTable(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Returns the ObjectName ScreeningTableMBean at the specified position in the array of all of the ScreeningTableMBeans associated with this OwnSignallingPointMBean.
getScreeningTables() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all of the ScreeningTableMBeans created by this layer manager.
getScreeningTables() - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Returns an array of ObjectNames of all the ScreeningTableMBeans associated with this OwnSignallingPointMBean.
getScreeningType() - Method in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  Returns the screening type option that is in use.
getServiceIndicator() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Returns the service indicator one of the service indicator constants.
getSharingMode() - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Returns the sharing mode used by this SCCP entity set.
getSignallingLinkCode() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Gets the Signalling Link Code (SLC) parameter of this Signalling Link.
getSignallingPoint() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Gets the ObjectName of the Signalling Point of this Service Access Point.
getSignallingPoint(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of one of the SignallingPointMBeans created by this layer manager
getSignallingPointCode() - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Gets the Signalling Point Code of this Signalling Point.
getSignallingPoints() - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Returns the ObjectNames of all the SignallingPointMBeans created by this layer manager
getStackName() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Returns the Stack Name.
getStatistic(Integer) - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Returns an OamStatisticNotification of the specified statistic type containing the value of the statistic.
getStatisticType() - Method in class jain.protocol.ss7.oam.OamStatisticNotification
  Returns the Type of this Statistic
getStatisticValue() - Method in class jain.protocol.ss7.oam.OamStatisticNotification
  Returns the value of the statistic being sent in this Statistic Notification.
getSubsystem(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns the ObjectName of one of the Subsystems (SCCP Access Points) associated with the SCCP Routing Control (local signalling Point).
getSubsystem(Integer) - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Returns the ObjectName of one of the subsystems of this TCAP Node
getSubsystemNumber() - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Gets the Subsystem Number of this SubsystemMBean.
getSubsystems() - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Returns an array of ObjectNames of all the Subsystems (SCCP Access Points) associated with the SCCP Routing Control (local signalling Point).
getSubsystems() - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Returns an array of ObjectNames of the set of subsystems of this TCAP Node
getSubsystemStatus() - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Indicates the status of the Local Subsystem.
getTcapNode(Integer) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Returns the ObjectName of one of the TCAP layers managed by this TCAP Layer Manager.
getTcapNodes() - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Returns an array of ObjectNames of all the TCAP layers managed by this TCAP Layer Manager.
getTimerId() - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Returns the Timer Id of the Timer that caused the Timer Expired Alarm [when ALARM_TIMER_EXPIRED == getAlarmType()].
getTimerId() - Method in interface jain.protocol.ss7.oam.OamTimerValMBean
  Returns the ID of the this timer value.
getTimestamp() - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Returns the timestamp indicating the time at which this alarm was emitted.
getTranslationType() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Gets the Translation Type of this Global Title Entry
getType() - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Returns the type of this Signalling point (one of the Signalling Type constants).
getValidList(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  Returns an array of ObjectNames representing either all of the allowed Linksets or all of the allowed Originating Point Codes for the specified destination point code.
  The type of Objects that is returned in the array of ObjectNames is dependent on the screening type option.
getVendorDetails() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Returns a String that identifies the Vendor that supplied this implementation.
GlobalTitleEntryMBean - interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean.
  This class represents a Global Title entry (a combination of the global title translator and global title rule).
GTINDICATOR_0001 - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  A Global title indicator constant: indicator = 0001
GTINDICATOR_0010 - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  A Global title indicator constant: indicator = 0010
GTINDICATOR_0011 - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  A Global title indicator constant: indicator = 0011
GTINDICATOR_0100 - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  A Global title indicator constant: indicator = 0100

## H

hasGlobalTitle(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Indicates if a Global Title (identified by the specified ObjectName) is assocaited with this SCCP.

## I

IllegalOperationException - exception jain.protocol.ss7.oam.IllegalOperationException.
  This Exception is thrown if a method has been invoked that is supported by the implementation, but cannot be performed given the current state of the system.
IllegalOperationException() - Constructor for class jain.protocol.ss7.oam.IllegalOperationException
  Constructs a new `IllegalOperationException`.
IllegalOperationException(String) - Constructor for class jain.protocol.ss7.oam.IllegalOperationException
  Constructs a new `IllegalOperationException` with the specified detail message.
initialiseTimers() - Method in interface jain.protocol.ss7.oam.OamTimerProfileMBean
  Initialises the timers to their default values.
isActive() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns whether this Signalling Link is active or innactive.
isAllLinksActive() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns whether all the Links in this Linkset are active or innactive.
isCombinedLinkSet() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns whether this Linkset is a combined Linkset
isEnabled() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns whether this Link is enabled or disabled (the operational state of this Link).
isEnabled() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns whether this Linkset is enabled or disabled (the operational state of this Linkset).
isLoadSharing() - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Indicates if this Routeset supports Load Sharing.
isLocallyBlocked() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the Locally Blocked Status parameter of this Signalling Link.
isLocked() - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Returns the Administrative state parameter of this Global Title Entry.
isRoutingAllowed() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Returns whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via the firstLinkset of this Route (the Adiministrative State).
isRoutingAllowed() - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Returns whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point of this Routeset (the Adiministrative State).
isRoutingAllowed() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via this Link (the Adiministrative State).
isRoutingAllowed() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Returns whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via this Linkset (the Adiministrative State).
isSignallingLinkTestOn() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns the Signalling Link testing.
isSignallingPointAccessible() - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Indicates if the respective Destination Signalling Point is accessible via the firstLinkset of this Route (the Operational State).
isSignallingPointAccessible() - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Indicates if the Destination Signalling Point of this Routeset is accessible (the Operational State).
isTestedPeriodically() - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  This attribute indicates whether the periodic test procedure of ITU Rec.
isTestPeriodically() - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Returns whether the link is tested periodically.

## J

jain.protocol.ss7 - package jain.protocol.ss7
  This package contains the JAIN SS7 Factory, which is the central creation point for all high level proprietary JAIN SS7 objects, for example JainTcapStack Objects.
jain.protocol.ss7.oam - package jain.protocol.ss7.oam
  This package contains the main interfaces and classes of the JAIN Operations, Administration and Maintenance API.
jain.protocol.ss7.oam.mtp2 - package jain.protocol.ss7.oam.mtp2
  This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 2 layer.
jain.protocol.ss7.oam.mtp3 - package jain.protocol.ss7.oam.mtp3
  This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 3 layer.
jain.protocol.ss7.oam.sccp - package jain.protocol.ss7.oam.sccp
  This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the SCCP layer.
jain.protocol.ss7.oam.tcap - package jain.protocol.ss7.oam.tcap
  This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the TCAP layer.
JainSS7Factory - class jain.protocol.ss7.JainSS7Factory.
  The JAIN(tm) SS7 Factory is a singleton class by which JAIN SS7 applications can obtain a proprietary (Peer) JAIN SS7 Object.
JainSS7Utility - class jain.protocol.ss7.JainSS7Utility.
JainSS7Utility() - Constructor for class jain.protocol.ss7.JainSS7Utility

## L

LinkMBean - interface jain.protocol.ss7.oam.mtp3.LinkMBean.
  This interface defines the methods of a Link Managed Bean.
LinkSetMBean - interface jain.protocol.ss7.oam.mtp3.LinkSetMBean.
  This interface defines the methods of a Linkset to an adjacent node.

## M

MTP2_ALARM_REMOTE_CONGESTION_START - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Remote end congestion started due to unknown cause.
MTP2_ALARM_REMOTE_CONGESTION_STOP - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Remote end congestion stopped.
MTP2_ALARM_RETRANSMIT_Q_FULL - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Retransmit queue full.
MTP2_ALARM_RETRANSMIT_Q_NOT_FULL - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Retransmit queue is no longer full.
MTP2_ALARM_SL_ABNORMAL_FIBR_BSNR - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Indicates a signalling link failure due to an abnormal FIBR or BSNR of a signalling link.
MTP2_ALARM_SL_ALIGNED - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link aligned.
MTP2_ALARM_SL_CONGESTION_START - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link entered congestion due to management initiated or unknown reason.
MTP2_ALARM_SL_CONGESTION_STOP - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link leaving congestion due to management initiated or unknown reason.
MTP2_ALARM_SL_DOWN_PHYSICAL - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link is down at physical level.
MTP2_ALARM_SL_EXCESSIVE_DELAY_ACK - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Indicates a signalling link failure due to an excessive delay of ack of a signalling link.
MTP2_ALARM_SL_NOT_ALIGNED - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link not aligned.
MTP2_ALARM_SL_START_REMOTE_PROCESSOR_OUTAGE - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Indicates the start of remote processor outage.
MTP2_ALARM_SL_UP_PHYSICAL - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Alarm Type Constant: Link is up at physical level.
MTP2_ERROR_INVALID_TIMER_EXPIRED - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2ErrorNotification
  Alarm Type Constant: Invalid MTP2 Timer Expired.
MTP2_MSU_DISCARD_SL_CONGESTION - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification
  A MTP2 Statistic Type constant: MSUs discarded due to SL congestion.
MTP2_NUM_SIF_SIO_RECIEVED - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification
  A MTP2 Statistic Type constant: Number of SIF and SIO octets received.
MTP2_NUM_SIF_SIO_TRANS - Static variable in class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification
  A MTP2 Statistic Type constant: Number of SIF and SIO octets transmitted.
Mtp2AlarmNotification - class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification.
  A Mtp2AlarmNotification is an Notification emitted by a Mtp2 Managed MBean(MBean) to indicate a change in status of the MBean.
Mtp2AlarmNotification(OamManagedObjectMBean, long, int, int) - Constructor for class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Constructs a new `Mtp2AlarmNotification`.
Mtp2ErrorNotification - class jain.protocol.ss7.oam.mtp2.Mtp2ErrorNotification.
  This Notification may be emitted by any MTP2 Managed MBean if a user defined error is encountered.
Mtp2ErrorNotification(OamManagedObjectMBean, long, int) - Constructor for class jain.protocol.ss7.oam.mtp2.Mtp2ErrorNotification
  Constructs a new Mtp2ErrorNotification of the specified Error Type.
Mtp2LayerManagerMBean - interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean.
  This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
Mtp2ManagedObjectMBean - interface jain.protocol.ss7.oam.mtp2.Mtp2ManagedObjectMBean.
  This interface is used by an MBean to emit three differect types of Mtp2 Notifications.
Mtp2SapMBean - interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean.
  This interface identifies an Mtp2 Service Access Point (SAP), an MTP2 SAP contains the attributes of the physical port and link that is connected to the logical signalling link.
Mtp2StatisticNotification - class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification.
  An Mtp2StatisticNotification is a Notification emitted by an Mtp2ManagedObjectMBean containing the value of a particular statistic.
Mtp2StatisticNotification(OamManagedObjectMBean, long, int, int, int) - Constructor for class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification
  Constructs a new `Mtp2StatisticNotification`.
Mtp2TimerProfileMBean - interface jain.protocol.ss7.oam.mtp2.Mtp2TimerProfileMBean.
  This interface defines the specified timers for the MTP2 Protocol Layer.
MTP3_ADJ_SP_INACCESSIBLE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Adjacent SP inaccessible.
MTP3_ALARM_CONCERNED_SP_NETWORK_CONGESTED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Concerned destination point code (DPC) network congested.
MTP3_ALARM_CONCERNED_SP_PAUSE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Concerned destination point code (DPC) pause.
MTP3_ALARM_CONCERNED_SP_RESUME - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Concerned destination point code (DPC) resume.
MTP3_ALARM_CONCERNED_SP_STOP_NET_CONG - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Concerned destination point code (DPC) stop network congestion.
MTP3_ALARM_CONCERNED_SP_USER_UNAVAILABLE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Concerned destination point code (DPC) remote user unavailable.
MTP3_ALARM_LS_BROADCAST_TFA - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the initiation of broedcast TFA due to the recovery of a measured linkset.
MTP3_ALARM_LS_BROADCAST_TFP - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the initiation of broedcast TFP due to failure of a measured linkset.
MTP3_ALARM_LS_CHANGE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the change in linkset used to adjacent Signalling Point.
MTP3_ALARM_LS_END_FAILURE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the end of Linkset failure.
MTP3_ALARM_LS_START_FAILURE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the start of Linkset failure.
MTP3_ALARM_RS_END_UNAVAILABILITY - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the end of unavailability of routeset to a given destination or set of destinations.
MTP3_ALARM_RS_START_UNAVAILABILITY - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Linkset and Routeset Availability: Indicates the start of unavailability of routeset to a given destination or set of destinations.
MTP3_ALARM_SL_END_REMOTE_PROCESSOR_OUTAGE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Availability: Indicates the end of remote processor outage.
MTP3_ALARM_SL_EXCESSIVE_CONGESTION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates a signalling link failure due to the excessive duration of congestion of a signalling link.
MTP3_ALARM_SL_EXCESSIVE_ERROR_RATE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates a signalling link failure due to an excessive error rate of a signalling link.
MTP3_ALARM_SL_FAILURE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates that there has been a signalling link failure.
MTP3_ALARM_SL_INHIBIT_DENIED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link inhibit denied.
MTP3_ALARM_SL_LOCAL_AUTO_CHANGEBACK - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates a local automatic changeback.
MTP3_ALARM_SL_LOCAL_AUTO_CHANGEOVER - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates a local automatic changeover.
MTP3_ALARM_SL_LOCALLY_BLOCKED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link locally blocked.
MTP3_ALARM_SL_LOCALLY_UNBLOCKED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link locally unblocked.
MTP3_ALARM_SL_REMOTELY_BLOCKED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link remotely blocked.
MTP3_ALARM_SL_REMOTELY_UNBLOCKED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link remotely unblocked.
MTP3_ALARM_SL_RESTORATION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Faults & Performance: Indicates the restoration of a signalling link.
MTP3_ALARM_SL_START_LOCAL_INHIBITION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Availability: Indicates the start of local inhibition.
MTP3_ALARM_SL_START_REMOTE_INHIBITION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Availability: Indicates the start of remote inhibition.
MTP3_ALARM_SL_STOP_LOCAL_INHIBITION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Availability: Indicates the stop of local inhibition.
MTP3_ALARM_SL_STOP_REMOTE_INHIBITION - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Signalling Link Availability: Indicates the stop of remote inhibition.
MTP3_ALARM_SL_UNINHIBIT_DENIED - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Link uninhibit denied.
MTP3_ALARM_SP_ACCESSIBLE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Mtp Signalling Point Status: Indicates that an adjacent Signalling Point is accessible.
MTP3_ALARM_SP_INACCESSIBLE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Alarm Type Constant: Mtp Signalling Point Status: Indicates that the adjacent Signalling Point is inaccessible.
MTP3_DUR_ADJ_SP_INACCESSIBLE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Duration of adjacent SP inaccessible.
MTP3_DUR_LINK_IN_SERV - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Duration of link in the In-service state.
MTP3_DUR_SL_UNAVAILABILITY - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Duration of SL unavailability (for any reason).
MTP3_DUR_UNAVAILABILITY - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Duration of unavailability of a routeset to a given destination or set of destinations.
MTP3_ERROR_ILLEGAL_TIMER_EXPIRY - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3ErrorNotification
  Illegal timer expiry in the MTP3 software.
MTP3_ERROR_ROUTING_ERROR - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3ErrorNotification
  Routing error.
MTP3_MSU_DISCARD_ROUTE_DATA_ERR - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: MSU discarded due to a routing data error.
MTP3_NUM_SIG_UNITS_RECEIVED_ERR - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Number of signal units received in error.
MTP3_SL_FAILURE - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: SL failure - All reasons.
MTP3_UNAVAILABILITY_ROUTE_SET - Static variable in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  A MTP3 Statistic Type constant: Unavailability of routeset to a given destination or set of destinations.
Mtp3AlarmNotification - class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification.
  A Mtp3AlarmNotification is a Notification emitted by a Mtp3 Managed Bean(MBean) to indicate a change in status of the MBean.
Mtp3AlarmNotification(OamManagedObjectMBean, long, int, int) - Constructor for class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Constructs a new `Mtp3AlarmNotification`.
Mtp3ErrorNotification - class jain.protocol.ss7.oam.mtp3.Mtp3ErrorNotification.
  This Notification may be emitted by any Mtp3 Managed Bean if a user defined error is encountered.
Mtp3ErrorNotification(OamManagedObjectMBean, long, int) - Constructor for class jain.protocol.ss7.oam.mtp3.Mtp3ErrorNotification
  Constructs a new Mtp3ErrorNotification of the specified Error Type.
Mtp3LayerManagerMBean - interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean.
  This interface defines the methods required for the creation and management of all MTP Level 3 Managed MBeans.
Mtp3ManagedObjectMBean - interface jain.protocol.ss7.oam.mtp3.Mtp3ManagedObjectMBean.
  This interface is used by an MBean to emit three differect types of Mtp3 Notifications.
Mtp3SapMBean - interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean.
  This interface identifies an Mtp3 Service Access Point (SAP).
Mtp3StatisticNotification - class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification.
  An Mtp3StatisticNotification is a Notification emitted by an Mtp3ManagedObjectMBean containing the value of a particular statistic.
Mtp3StatisticNotification(OamManagedObjectMBean, long, int, int, int) - Constructor for class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  Constructs a new `Mtp3StatisticNotification`.
Mtp3TimerProfileMBean - interface jain.protocol.ss7.oam.mtp3.Mtp3TimerProfileMBean.
  This interface defines the specified timers for the MTP3 Protocol Layer .

## N

NA_INTERNATIONAL - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Nature of Address Indicator constant: Indicates an international number.
NA_NATIONAL_SIGNIFICANT - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Nature of Address Indicator constant: Indicates a National Significant Number.
NA_RESERVED - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Nature of Address Indicator constant: Reserved for national use.
NA_SUBSCRIBER - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Nature of Address Indicator constant: Indicates a subsciber number.
NA_UNKNOWN - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Nature of Address Indicator constant: Indicates a unknown Nature of Address Indicator.
NI_INTERNATIONAL_00 - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A Network Indicator constant: Indicates the International Network 00, this has an integer value of 0.
NI_INTERNATIONAL_00 - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Network indicator constant.
NI_INTERNATIONAL_01 - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A Network Indicator constant: Indicates the International Network 01, this has an integer value of 1.
NI_INTERNATIONAL_01 - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Network indicator constant.
NI_NATIONAL_10 - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A Network Indicator constant: Indicates the National Network 10, this has an integer value of 2.
NI_NATIONAL_10 - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Network indicator constant.
NI_NATIONAL_11 - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A Network Indicator constant: Indicates the National Network 11, this has an integer value of 3.
NI_NATIONAL_11 - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Network indicator constant.
NON_OAM_RELATED_ERROR - Static variable in class jain.protocol.ss7.oam.OamErrorNotification
  Eror Type constant: Indicates that a non-OAM related.
NP_DATA - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Data Numbering Plan.
NP_GENERIC - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Generic Numbering Plan.
NP_ISDN_MOBILE - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: ISDN/Mobile Numbering Plan.
NP_ISDN_TEL - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: ISDN/Telephony Numbering Plan.
NP_LAND_MOBILE - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Land/Mobile Numbering Plan.
NP_MARITIME_MOBILE - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Maritime Mobile Numbering Plan.
NP_NETWORK - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Private Network or Network Specific Numbering Plan.
NP_TELEX - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Telex Numbering Plan.
NP_UNKOWN - Static variable in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Numbering Plan Constant: Unkown Numbering Plan.

## O

OamAlarmNotification - class jain.protocol.ss7.oam.OamAlarmNotification.
  An OamAlarmNotification is a Notification emitted by a JAIN OAM Layer Manager MBean to indicate a change in status of the MBean.
OamErrorNotification - class jain.protocol.ss7.oam.OamErrorNotification.
  This Notification may be emitted by any OAMLayerManagerMBean object if an error is encountered.
OamLayerManagerMBean - interface jain.protocol.ss7.oam.OamLayerManagerMBean.
  This interface defines the methods common to all Protocol Layer Managers.
OamLookupTable - interface jain.protocol.ss7.oam.OamLookupTable.
  This interface provides a mechanism for an application to map between a MBean's ObjectName and a reference.
OamManagedObjectMBean - interface jain.protocol.ss7.oam.OamManagedObjectMBean.
  This interface is implemented by all JAIN OAM Managed Beans (MBeans).
OamStatisticNotification - class jain.protocol.ss7.oam.OamStatisticNotification.
  An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
OamTimerProfileMBean - interface jain.protocol.ss7.oam.OamTimerProfileMBean.
  An Oam Timer Profile is used to store all the OAM Timer Values for a particular Protocol Layer.
OamTimerValMBean - interface jain.protocol.ss7.oam.OamTimerValMBean.
  This interface represents an individual SS7 timer.
OBJECT_TYPE_CONCERNED_AREA - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a ConcernedAreaMBean, getObjectType() for this MBean returns "OBJECT_TYPE_CONCERNED_AREA".
OBJECT_TYPE_GLOBAL_TITLE_ENTRY - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a GlobalTitleEntryMBean, getObjectType() for this MBean returns "OBJECT_TYPE_GLOBAL_TITLE_ENTRY".
OBJECT_TYPE_LINK - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a LinkMBean, getObjectType() for this MBean returns "OBJECT_TYPE_LINK".
OBJECT_TYPE_LINKSET - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a LinksetMBean, getObjectType() for this MBean returns "OBJECT_TYPE_LINKSET".
OBJECT_TYPE_MTP2_LAYER_MANAGER - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp2LayerManager, getObjectType() for this MBean returns "OBJECT_TYPE_MTP2_LAYER_MANAGER".
OBJECT_TYPE_MTP2_SAP - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp2SapMBean, getObjectType() for this MBean returns "OBJECT_TYPE_MTP2_SAP".
OBJECT_TYPE_MTP2_TIMER_PROFILE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp2TimerProfileMBean, getObjectType() for this MBean returns "OBJECT_TYPE_MTP2_TIMER_PROFILE".
OBJECT_TYPE_MTP3_LAYER_MANAGER - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp3LayerManager, getObjectType() for this MBean returns "OBJECT_TYPE_MTP3_LAYER_MANAGER".
OBJECT_TYPE_MTP3_SAP - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp3SapMBean, getObjectType() for this MBean returns "OBJECT_TYPE_MTP3_SAP".
OBJECT_TYPE_MTP3_TIMER_PROFILE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a Mtp3TimerProfileMBean, getObjectType() for this MBean returns "OBJECT_TYPE_MTP3_TIMER_PROFILE".
OBJECT_TYPE_OAM_TIMER_VAL - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a OamTimerValMBean, getObjectType() for this MBean returns "OBJECT_TYPE_OAM_TIMER_VAL".
OBJECT_TYPE_OWN_SIGNALLING_POINT - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for an OwnSignallingPointMBean, getObjectType() for this MBean returns "OBJECT_TYPE_OWN_SIGNALLING_POINT".
OBJECT_TYPE_ROUTE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a RouteMBean, getObjectType() for this MBean returns "OBJECT_TYPE_ROUTE".
OBJECT_TYPE_ROUTESET - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a RoutesetMBean, getObjectType() for this MBean returns "OBJECT_TYPE_ROUTESET".
OBJECT_TYPE_SCCP_ENTITY_SET - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a SccpEntitySetMBean, getObjectType() for this MBean returns "OBJECT_TYPE_SCCP_ENTITY_SET".
OBJECT_TYPE_SCCP_LAYER_MANAGER - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a SccpLayerManager, getObjectType() for this MBean returns "OBJECT_TYPE_SCCP_LAYER_MANAGER".
OBJECT_TYPE_SCCP_ROUTING_CONTROL - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a SccpRoutingControlMBean, getObjectType() for this MBean returns "OBJECT_TYPE_SCCP_ROUTING_CONTROL".
OBJECT_TYPE_SCCP_SAP - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a SccpSapMBean, getObjectType() for this MBean returns "OBJECT_TYPE_SCCP_SAP".
OBJECT_TYPE_SCCP_TIMER_PROFILE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a SccpTimerProfileMBean, getObjectType() for this MBean returns "OBJECT_TYPE_SCCP_TIMER_PROFILE".
OBJECT_TYPE_SCREENING_TABLE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a ScreeningTableMBean, getObjectType() for this MBean returns "OBJECT_TYPE_SCREENING_TABLE".
OBJECT_TYPE_TCAP_LAYER_MANAGER - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a TcapLayerManager, getObjectType() for this MBean returns "OBJECT_TYPE_TCAP_LAYER_MANAGER".
OBJECT_TYPE_TCAP_NODE - Static variable in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  The Object Type for a TcapNodeMBean, getObjectType() for this MBean returns "OBJECT_TYPE_TCAP_NODE".
OwnSignallingPointMBean - interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean.
  This interface defines the methods of a Local Signalling Point Managed Bean(MBean).

## P

PORT_TYPE_DCE - Static variable in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  A port clocking type constant: Indicates that the port connects the transmit clock to an internal baud rate generator and provides this clock to the applicable line interface circuit.
PORT_TYPE_DTE - Static variable in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  A port clocking type constant: Indicates that the port connects the transmit clock to the applicable line interface circuit.
PRIORITY_CRITICAL - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Indicates that this is a Critical Alarm.
PRIORITY_HIGH - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Indicates that this is a High Priority Alarm.
PRIORITY_INFORMATIONAL - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Indicates that this is an Informational Alarm.
PRIORITY_LOW - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Indicates that this is a Low Priority Alarm.
PRIORITY_VENDOR_DEFINED - Static variable in class jain.protocol.ss7.oam.OamAlarmNotification
  Indicates that this alarm has a severity that is defined by the SS7 stack vendor.
PROTOCOL_VARIANT_ANSI_1992 - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  A Protocol Version constant: ANSI Protocol
PROTOCOL_VARIANT_ANSI_1996 - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
PROTOCOL_VARIANT_ITU_1993 - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  A Protocol Version constant: ITU Protocol
PROTOCOL_VARIANT_ITU_1996 - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
PROTOCOL_VARIANT_ITU_1997 - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
PROTOCOL_VARIANT_OTHER - Static variable in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  A Protocol Version constant: a protocol other then ITU or ANSI
put(ObjectName, Object) - Method in interface jain.protocol.ss7.oam.OamLookupTable
  Adds an ObjectName/object reference pair to the table.

## R

ReadConfigurationException - exception jain.protocol.ss7.oam.ReadConfigurationException.
  This Exception is thrown by a JAIN OAM Layer object if the readCurrentConfiguration() method has been invoked and an error is encountered while attempting to establish the current system configuration or while creating the Managed MBeans that represent the current system configuration.
ReadConfigurationException() - Constructor for class jain.protocol.ss7.oam.ReadConfigurationException
  Constructs a new `ReadConfigurationException`.
ReadConfigurationException(String) - Constructor for class jain.protocol.ss7.oam.ReadConfigurationException
  Constructs a new `ReadConfigurationException` with the specified detail message.
readCurrentConfiguration() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Gets the current configuration of the SS7 Layer being managed.
remove(ObjectName) - Method in interface jain.protocol.ss7.oam.OamLookupTable
  Removes an ObjectName/object reference pair from the table.
removeNotificationListenerFromAllMBeans(NotificationListener) - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Removes the specified NotificationListener from listening to all of the OamManagedObjectMBeans of this Layer Manager.
rollBack() - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Resets the MBeans back to the state they were in after the last call to the commit() or readCurrentConfiguration().
ROUTE_AVAILABLE - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Indicates that this Route is available.
ROUTE_RESTRICTED - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Indicates that this Route is restricted.
ROUTE_UNAVAILABLE - Static variable in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Indicates that this Route is unavailable.
RouteMBean - interface jain.protocol.ss7.oam.mtp3.RouteMBean.
  This interface defines the methods of a Route Managed Bean (RouteMBean).
RouteSetMBean - interface jain.protocol.ss7.oam.mtp3.RouteSetMBean.
  This interface defines the methods of a Routeset Managed Bean (RouteSetMBean).

## S

SCCP_ALARM_QOS_HOP_COUNTER_VIOLATION - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Hop Counter Violation.
SCCP_ALARM_QOS_NO_REASSEBLY_SPACE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: No Reassembly Space.
SCCP_ALARM_QOS_NO_RULE_FOR_ADDR - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: No Rule For Address .
SCCP_ALARM_QOS_NO_SEGEMENTATION_SUPPORT - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: No Segmentation Support .
SCCP_ALARM_QOS_NO_TRANSLATOR_FOR_ADDR - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Alarm Type Constant: No Translator For Address ).
SCCP_ALARM_QOS_PC_CONGESTED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Point Code Congested .
SCCP_ALARM_QOS_PC_NOT_AVAILABLE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Point Code Not Available .
SCCP_ALARM_QOS_REASSEMBLY_FAILURE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Reassembly Failure.
SCCP_ALARM_QOS_REASSEMBLY_TIMEOUT - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Reassembly TimeOut .
SCCP_ALARM_QOS_ROUTING_FAILURE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Routing Failure (no reason or unqualified).
SCCP_ALARM_QOS_SEGMENT_OUT_OF_ORDER - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Segment Out Of Order .
SCCP_ALARM_QOS_SEGMENTATION_FAILURE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Segmentation Failure.
SCCP_ALARM_QOS_SSN_CONGESTED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Subsystem Congested .
SCCP_ALARM_QOS_SSN_UNAVAILABLE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Subsystem Unavailable.
SCCP_ALARM_QOS_SSN_UNEQUIPED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Unequiped Subsystem).
SCCP_ALARM_QOS_SYNTAX_ERROR - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Syntax Error Detected .
SCCP_ALARM_QOS_TOO_LARGE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Quality Of Service: Too Large For Segmentation.
SCCP_ALARM_SSN_ALLOWED_RX - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates that a Subsystem allowed message has been received.
SCCP_ALARM_SSN_AVAILABLE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates that a local SCCP has become available, after being unavailable for any reason.
SCCP_ALARM_SSN_END_PROHIBITED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates the end of a Subsystem prohibited.
SCCP_ALARM_SSN_OOS_DENIED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates that a subsystem of out-of-service request has been denied.
SCCP_ALARM_SSN_OOS_GRANT - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates that a subsystem of out-of-service grant message has benn received.
SCCP_ALARM_SSN_START_PROHIBITED - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates the start of a Subsystem prohibited.
SCCP_ALARM_SSN_UNAVAILABLE_CONGESTION - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates the start of a local SCCP unavailable due to congestion.
SCCP_ALARM_SSN_UNAVAILABLE_FAILURE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates the start of a local SCCP unavailable due to failure.
SCCP_ALARM_SSN_UNAVAILABLE_MAINTENANCE - Static variable in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Alarm Type Constant: Sccp Subsystem Availability: Indicates the start of a local SCCP unavailable due to maintenance.
SCCP_ERROR_ILLEGAL_TIMER_EXPIRY - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Illegal timer expiry in the SCCP software.
SCCP_ERROR_MSG_DECODING - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Error encountered while decoding SCCP message.
SCCP_ERROR_MSG_INVALID - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Invalid network message.
SCCP_ERROR_MSG_INVALID_TYPE - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Invalid message type.
SCCP_ERROR_MSG_PARAM_OUT_OF_RANGE - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Parameter in a message is out of range.
SCCP_ERROR_MSG_SYNTAX - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Syntax error in message received from the network.
SCCP_ERROR_ROUTING_ERROR - Static variable in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Routing error - Invalid route or route not available.
SCCP_FAIL_OF_RELEASE_COMPLETE_SUPERVISION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Failure of release complete supervision.
SCCP_HOP_COUNTER_VIOLATION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Hop counter violation (XUDT, XUDTS, LUDT, LUDTS and CR).
SCCP_MSG_TOO_LARGE_FOR_SEG - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Message too large for segmentation.
SCCP_PROVIDER_INI_RELEASE_OF_CONNECTION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Provider initiated release of a connection.
SCCP_PROVIDER_INI_RESET_OF_A_CONNECTION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Provider initiated reset of a connection.
SCCP_REASSEMBLY_ERR_SEG_RECEIVED_OUT_OF_SEQ - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Reassembly error - Segment received out of sequence (including duplicates, recpt, of non-first segment for which no reassembly process).
SCCP_REASSEMBLY_ERR_TIME_T_REASS_EXPIRY - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Reassembly error - Timer The timer returned by getSccpTimerReassembly() has expired.
SCCP_REASSEMBLY_ERROR_NO_REASSEMBLY_SPACE - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Reassembly error - No reassembly space.
SCCP_ROUTING_FAIL_NETWORK_CONGESTION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Network Congestion.
SCCP_ROUTING_FAIL_NETWORK_FAILURE - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Network Failure (Point Code not available).
SCCP_ROUTING_FAIL_NO_TRANS_FOR_ADD - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - No translation for address of such nature.
SCCP_ROUTING_FAIL_NO_TRANS_FOR_THIS_SPEC_ADD - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - No translation for this specific address.
SCCP_ROUTING_FAIL_SUBSYSTEM_CONGESTION - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Subsystem Congestion.
SCCP_ROUTING_FAIL_SUBSYSTEM_FAIL - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Subsystem Failure (unavailable).
SCCP_ROUTING_FAIL_UNEQUIPPED_USER - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Unequipped user (Subsystem).
SCCP_ROUTING_FAIL_UNQUALIFIED - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Routing Failure - Unqualified.
SCCP_SEG_ERR_SEG_FAIL - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Segmentation error - Segmentation failed.
SCCP_STATUS_ALLOWED - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A Subsystem Status constant: The local Subsystem has registered and become Allowed
SCCP_STATUS_PROHIBITED - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A Subsystem Status constant: The Subsystem has registered (is equipped) but has not yet become allowed, or is prohibited.
SCCP_STATUS_UNEQUIPPED - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A Subsystem Status constant: The Subsystem has not registered to the SCCP layer, the Subsystem has deregistered, or the Subsystem has failed.
SCCP_SYNTAX_ERROR_DETECTED - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Syntax Error Detected.
SCCP_TIMER_T_IAR_EXPIRY - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Timer The timer returned by getSccpTimerIAR() has expired.
SCCP_UDT_ORIG_CLASS_SSN - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Total (L)(X)UDT messages originated per class and source SSN.
SCCP_UDT_TERM_CLASS_SSN - Static variable in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  A SCCP Statistic Type constant: Total (L)(X)UDT messages terminated per class and sink SSN.
SccpAlarmNotification - class jain.protocol.ss7.oam.sccp.SccpAlarmNotification.
  A SccpAlarmNotification is an Notification emitted by a Sccp Managed Bean (MBean) to indicate a change in status of the MBean.
SccpAlarmNotification(OamManagedObjectMBean, long, int, int) - Constructor for class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Constructs a new `SccpAlarmNotification`.
SccpEntitySetMBean - interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean.
  This class identifies the set of access points that result from a global title translation.
SccpErrorNotification - class jain.protocol.ss7.oam.sccp.SccpErrorNotification.
  This Notification may be emitted by any Sccp Managed MBean if a user defined error is encountered.
SccpErrorNotification(OamManagedObjectMBean, long, int) - Constructor for class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Constructs a new SccpErrorNotification of the specified Error Type.
SccpLayerManagerMBean - interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean.
  This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
SccpManagedObjectMBean - interface jain.protocol.ss7.oam.sccp.SccpManagedObjectMBean.
  This interface is used by an MBean to emit three differect types of Sccp Notifications.
SccpRoutingControlMBean - interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean.
  This interface defines the methods required by the SCCP Routing Control Function It defines methods to maintain management information concerning the SCCP routing control.
SccpSapMBean - interface jain.protocol.ss7.oam.sccp.SccpSapMBean.
  This interface defines a SCCP Access Point (an SCCP Subsystem).
SccpStatisticNotification - class jain.protocol.ss7.oam.sccp.SccpStatisticNotification.
  An SccpStatisticNotification is a Notification emitted by an SccpManagedObjectMBean containing the value of a particular statistic.
SccpStatisticNotification(OamManagedObjectMBean, long, int, int, int) - Constructor for class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  Constructs a new `SccpStatisticNotification`.
SccpTimerProfileMBean - interface jain.protocol.ss7.oam.sccp.SccpTimerProfileMBean.
  This interface defines the specified timers for the SCCP Protocol Layer.
SCR_TYPE_INCOMING_LS_TO_DPC - Static variable in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  To inhibit/allow STP access by a combination of designated incoming link sets to designated DPCs.
SCR_TYPE_OPC_TO_DPC - Static variable in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  To inhibit/allow STP access by examination of OPC and DPC combination in the incoming STP message.
SCR_TYPE_OUTGOING_LS_TO_DPC - Static variable in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  To inhibit/allow STP access by a combination of designated outgoing link sets to designated DPCs.
ScreeningTableMBean - interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean.
  This interface defines the methods of an STP Screening Table Managed Bean(MBean).
setActive(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Activates or deactivates this Signalling Link.
setActiveLinkCount(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the number of links that should be active (alligned and ready for service) in this Linkset at all times.
setActiveMtp2Sap(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Sets one of the Mtp2 Service Access Points (Mtp2SapMBeans) identified by the specified ObjectName
setActiveMtp2Saps(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2LayerManagerMBean
  Sets all of the Mtp2 Service Access Points (Mtp2SapMBeans) identified by the specified array of ObjectNames
setActiveOwnSignallingPoint(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Sets one of the active (local) OwnSignallingPointMBeans of this stack.
  The underlying stack management system may support multiple signalling points on the the same system.
setActiveOwnSignallingPoints(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3LayerManagerMBean
  Sets all of the active (local) OwnSignallingPointMBeans of this stack.
  The underlying stack management system may support multiple Signalling points on the the same system.
setActiveSccpRoutingControl(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Sets one of the Active SCCP Routing controls (identified by the specified ObjectName) of this SCCP Layer Manager.
setActiveSccpRoutingControls(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpLayerManagerMBean
  Sets the Active SCCP Routing controls (identified by the specified ObjectName) of this SCCP Layer Manager.
setActiveTcapNode(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Sets one of the active TCAP layers (identified by the specified ObjectName) managed by this TCAP Layer Manager.
setActiveTcapNodes(ObjectName[]) - Method in interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean
  Sets all of the active TCAP layers (identified by the specified array of ObjectNames) managed by this TCAP Layer Manager.
setAddressInformation(Byte[]) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Address Information of this Global Title Entry.
setAdjacentSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the Adjacent OwnSignallingPointMBean (identified by the specified ObjectName) of this LinksetMBean.
setAllLinksActive(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Activates or deactivates all the Links in this Linkset.
setBackup(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets the Backup OwnSignallingPointMBean of this OwnSignallingPointMBean identified by the specified ObjectName.
setCategory(int) - Method in class jain.protocol.ss7.oam.OamStatisticNotification
  Returns the category of this OamStatisticNotification.
setCombinedLinkSet(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the LinksetMBean at the specified position in the combined linkset of this linkset
setCombinedLinkSets(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the combined Linkset of this linkset
setConcernedArea(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Sets the concerned area to be used by SCCP Management for broadcasting the SCCP status after completion of SCCP Restart.
setCongestionAbate(Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the value at which a link congestion situation ends for the specified congestion level.
setCongestionOnset(Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the value at which a link congestion situation starts for the specified congestion level.
setCurrentVal(Long) - Method in interface jain.protocol.ss7.oam.OamTimerValMBean
  This method sets the current value for this timer in milliseconds.
setDestinationSubsystem(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sets one of the destination Subsystems (SCCP SAPs) of this Entity Setidentified by the specified ObjectName.
setDestinationSubsystems(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sets the destination Subsystems (SCCP SAPs) of this Entity Set identified by the specified ObjectName.
setDestSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Sets the Service Access Point (Mtp3SapMBean) that identifies the Destination OwnSignallingPointMBean (identified by the specified ObjectName) of this Routeset.
setDiscardAbate(Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the value at which MSUs are no longer discarded for the specified discard level.
setDiscardOnset(Integer, Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the value at which MSUs are discarded for the specified discard level.
setEnabled(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the operational state of this link.
setEnabled(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the operational state of this Linkset.
setEncodingScheme(Integer) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Encoding Scheme of this Global Title Entry.
setGlobalTitleEntries(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Sets the list of Global Title Entries associated with this Routing Control.
setGlobalTitleEntry(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Set this Global Title Entry as the specified element in the Global Title Entry Array of this Routing Control.
setGTIndicator(Integer) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Global Title indicator.
setInstalled(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Installed Status parameter of this Signalling Link.
setLink(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the Signalling LinkMBean at the specified position in the set of links of this linkSetMBean
setLinkNormal(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Link Normal Status parameter of this Signalling Link.
setLinks(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the Signalling Links of this linkset
setLinkSet(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Sets a Linkset at the specified position in the Linkset (identified by the specified ObjectName) in this route
setLinkSets(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Sets the Linksets in this route identified by the specified ObjectName
setLoadSharing(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Sets whether or not this Routeset supports Load Sharing.
setLocallyBlocked(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Locally Blocked Status parameter of this Signalling Link.
setLocked(Boolean) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Administrative state of this Global Title Entry.
setMaxCapacity(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets the Maximum Capacity of this Linkset.
setMtp2Sap(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Mtp2 Service Access Point MBean (identified by the specified ObjecName) associated with this Signalling Link (LinkMBean).
setMtp2TimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  Sets the MTP2 Timer Profile MBean (specified by its ObjectName) containing the MTP2 Timer values to be used with this link.
setMtp3Sap(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Sets the MTP3 Access Point representing the Signalling Point (MTP) used by this SCCP.
setMtp3TimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets the Mtp3TimerProfileMBean (identified by the specified ObjectName) containing the MTP3 Timer values to be used with this OwnSignallingPointMBean
setName(String) - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Sets the name of this OamManagedBean.
setNatureOfAddrInd(Integer) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Nature of Address Indicator of this Global Title Entry.
setNetworkIndicator(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Sets the Network Indicator parameter of this Signalling Point (one of the Network Indicator constants).
setNonOamErrorMsg(String) - Method in class jain.protocol.ss7.oam.OamErrorNotification
  Sets a non-OAM related error message.
setNumberingPlan(Integer) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Numbering Plan of this Global Title Entry.
setOwnSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Sets the local Signalling Point (identified by the specified ObjectName) governed by this routing control.
setOwnSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Sets the signalling point of this TCAP Node identified by the specified ObjectName.
setPathName(String) - Method in class jain.protocol.ss7.JainSS7Factory
  Sets the Pathname that identifies the location of a particular Vendor's implementation of the JAIN SS7 Objects.
setPortType(Integer) - Method in interface jain.protocol.ss7.oam.mtp2.Mtp2SapMBean
  Sets the clocking type of this port (DTE or DCE).
setPriority(int) - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Sets the Priority of this Alarm.
setPriority(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Sets the priority of this Route within the containing Routeset.
setProtocolVariantAndYear(Integer) - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Sets the protocol variant and year of the SS7 Protocol Layer represented by this OamLayerManager.
setRemoteSubsystem(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.ConcernedAreaMBean
  Sets one of the Remote Subsystems to be informed of local or remote subsystem status changes.
setRemoteSubsystems(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.ConcernedAreaMBean
  Sets all of the Subsystems (identified by the specified array of ObjectNames) to be informed of local or remote subsystem status changes.
setRoute(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Sets the route (identified by the specified ObjectName) at the specified position in this routeset.
setRoutes(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Sets the array of Routes (identified by the specified ObjectName) in this routeset.
setRouteSet(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets the RouteSetMBean (identified by the specified ObjectName) to the set of RouteSetMBeans of this OwnSignallingPointMBean at the the specified position
setRouteSets(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets all of the RouteSetMBeans associated with this OwnSignallingPointMBean.
setRoutingAllowed(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.RouteMBean
  Sets whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via the firstLinkset of this Route (the Adiministrative State).
setRoutingAllowed(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.RouteSetMBean
  Sets whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point of this Routeset (the Adiministrative State).
setRoutingAllowed(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via this Link (the Adiministrative State).
setRoutingAllowed(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkSetMBean
  Sets whether it is administratively permitted to route SS7 MSUs towards the Destination Signalling Point via this Linkset (the Adiministrative State).
setSccpEntitySet(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Entity Set of this GlobalTitle Entry identified by the specified ObjectName.
setSccpTimerProfile(ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Sets the SCCP Timer Profile containing the SCCP Timer values
setScreeningTable(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets the ScreeningTablesMBean (identified by the specified ObjectName) at the specified position in the array of all of the ScreeningTablesMBeans associated with this OwnSignallingPointMBean.
setScreeningTables(ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.OwnSignallingPointMBean
  Sets all of the ScreeningTablesMBeans associated with this OwnSignallingPointMBean.
setScreeningType(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  Sets the screening Type option to be used.
setServiceIndicator(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Sets the service indicator (one of the service indicator constants).
setSharingMode(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sets the sharing mode used by this SCCP entity set.
setSignallingLinkCode(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Signalling Link Code (SLC)of this Signalling Link.
setSignallingLinkTestOn(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the Signalling Link testing.
setSignallingPoint(ObjectName) - Method in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Sets the Signalling Point of this Service Access Point.
setSignallingPointCode(Long) - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Sets the Signalling Point Code of this Signalling Point.
setStackName(String) - Method in interface jain.protocol.ss7.oam.OamLayerManagerMBean
  Sets the Name of this Stack.
setStatisticValue(int) - Method in class jain.protocol.ss7.oam.OamStatisticNotification
  Sets the value of the statistic being sent in this Statistic Notification.
setStatus(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the status of this Link (as defined in ITU Rec.
setSubsystem(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Sets one of the Subsystems (SCCP Access Points) associated with the SCCP Routing Control (local signalling Point).
setSubsystem(Integer, ObjectName) - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Sets one of the subsystems (identified by the specified ObjectName of a SccpSapMBean) of this TCAP Node.
setSubsystemNumber(Integer) - Method in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  Sets the Subsystem Number of this SubsystemMBean.
setSubsystems(ObjectName[]) - Method in interface jain.protocol.ss7.oam.sccp.SccpRoutingControlMBean
  Sets all of the Subsystems (SCCP Access Points) associated with the SCCP Routing Control (local signalling Point).
setSubsystems(ObjectName[]) - Method in interface jain.protocol.ss7.oam.tcap.TcapNodeMBean
  Sets all of the subsystems (identified by the specified array of ObjectNames of SccpSapMBeans) of this TCAP Node.
setTestPeriodically(Boolean) - Method in interface jain.protocol.ss7.oam.mtp3.LinkMBean
  Sets the periodic testing of this signalling link
setTimerId(int) - Method in class jain.protocol.ss7.oam.OamAlarmNotification
  Sets the Timer Id that indicates the Timer that caused a Timer Expired Notification.
setTranslationType(Byte) - Method in interface jain.protocol.ss7.oam.sccp.GlobalTitleEntryMBean
  Sets the Translation Type of this Global Title Entry
setType(Integer) - Method in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  Sets the type of this Signalling Point (one of the Signalling Type constants).
setValidList(ObjectName, ObjectName[]) - Method in interface jain.protocol.ss7.oam.mtp3.ScreeningTableMBean
  Sets an array of Objects representing either: all of the allowed Linksets, or all of the allowed Originating Point Codes for the specified destination point code.
  The type of Object that is supplied in the Object array (identified from the array of ObjectNames) is dependent on the screening type option.
SI_BROADBAND_ISUP - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates broadband ISDN User Part.
SI_DUP_CALL_CIRCUIT - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates Data User Part - call and circuit-related messages.
SI_DUP_FACILITY_CANCELLATION - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates Data User Part - facility registration and cancellation messages.
SI_ISUP - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates ISDN User Part
SI_MTP_TESTING - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates reserved for MTP Testing User Part.
SI_SATELLITE_ISUP - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates satellite ISDN User Part.
SI_SCCP - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates SCCP.
SI_SIG_NET_MAN_MESSAGES - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates signalling network management messages.
SI_SIG_NET_TEST_MAIN_MESSAGES - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates signalling network testing and maintenance messages.
SI_TUP - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  Service Indicator constant: Indicates Telephone User Part.
SignallingPointMBean - interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean.
  This interface identifies an Signalling Point.
SM_DUPLI_DOMINANT - Static variable in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sharing Mode Constant: "Dupli-Dominant", indicates that the second entity is a backup for the first entity.
SM_DUPLI_REPLACEMENT - Static variable in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sharing Mode Constant: "Dupli-Replacement", indicates the second entity is standby for backup for the first entity, but after changeover, the primary and backup roles are swapped.
SM_DUPLI_SHARED - Static variable in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sharing Mode Constant: "Dupli-Loadshared", indicates that the load is shared over both the entities in the set.
SM_SOLITARY - Static variable in interface jain.protocol.ss7.oam.sccp.SccpEntitySetMBean
  Sharing Mode Constant: "Solitary", indicates that there can only be one access point in the set.
SS7Exception - exception jain.protocol.ss7.SS7Exception.
  This JAIN SS7 Exception is thrown when a general JAIN SS7 Error is encountered, and may be used when no other specific JainSS7 Excepion is relevant.
SS7Exception() - Constructor for class jain.protocol.ss7.SS7Exception
  Constructs a new Jain SS7 Exception
SS7Exception(String) - Constructor for class jain.protocol.ss7.SS7Exception
  Constructs a new Jain SS7 Exception with the specified detail message.
SS7ListenerAlreadyRegisteredException - exception jain.protocol.ss7.SS7ListenerAlreadyRegisteredException.
  This exception is thrown if the add Jain Listener method of a Jain Provider is invoked to add a Jain Listener to the list of registered Event Listeners, and the Jain Listener to be added is already a current registered Event Listener.
SS7ListenerAlreadyRegisteredException() - Constructor for class jain.protocol.ss7.SS7ListenerAlreadyRegisteredException
  Constructs a new `ListenerNotRegisteredException`
SS7ListenerAlreadyRegisteredException(String) - Constructor for class jain.protocol.ss7.SS7ListenerAlreadyRegisteredException
  Constructs a new `ListenerNotRegisteredException` with the specified detail message.
SS7ListenerNotRegisteredException - exception jain.protocol.ss7.SS7ListenerNotRegisteredException.
  This exception is thrown if the remove Jain Listener method of a Jain Provider is invoked to remove a Jain Listener from he list of registered Event Listeners, and the Jain Listener to be removed is not currently a registered Event Listener.
SS7ListenerNotRegisteredException() - Constructor for class jain.protocol.ss7.SS7ListenerNotRegisteredException
  Constructs a new `ListenerNotRegisteredException`
SS7ListenerNotRegisteredException(String) - Constructor for class jain.protocol.ss7.SS7ListenerNotRegisteredException
  Constructs a new `ListenerNotRegisteredException` with the specified detail message.
SS7PeerUnavailableException - exception jain.protocol.ss7.SS7PeerUnavailableException.
  The SS7 Peer Unavailable Exception indicates that the JAIN SS7 Peer (a particular implementation of JAIN SS7) is unavailable on the current system.
SS7PeerUnavailableException() - Constructor for class jain.protocol.ss7.SS7PeerUnavailableException
  Constructs a new SS7 Peer Unavailable Exception.
SS7PeerUnavailableException(String) - Constructor for class jain.protocol.ss7.SS7PeerUnavailableException
  Constructs a new SS7 Peer Unavailable Exception with the specified message detail.
startPollingStatistic(Integer, Integer) - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Initiates the polling of statistic of the specified statistic type on this OamManagedObjectMBean.
StatisticNotSupportedException - exception jain.protocol.ss7.oam.StatisticNotSupportedException.
  This Exception is thrown if the collection of a statistic that is not supported by the underlying Stack management system has been requested.
StatisticNotSupportedException() - Constructor for class jain.protocol.ss7.oam.StatisticNotSupportedException
  Constructs a new `StatisticNotSupportedException`.
StatisticNotSupportedException(String) - Constructor for class jain.protocol.ss7.oam.StatisticNotSupportedException
  Constructs a new `StatisticNotSupportedException` with the specified detail message.
STATUS_ALLOWED - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A SAP Status constant: Indicates that the status of the Access Point is Allowed.
STATUS_AVAILABLE - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A SCCP SAP Availability Status constant: Indicates that the status of the Access Point is Available.
STATUS_CONGESTED - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A SAP Status constant: Indicates that the status of the Access Point is Congested.
STATUS_DEGRADED - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A SCCP SAP Availability Status constant: Indicates that the status of the Access Point is Congested.
STATUS_PROHIBITED - Static variable in interface jain.protocol.ss7.oam.mtp3.Mtp3SapMBean
  A SAP Status constant: Indicates that the status of the Access Point is Prohibited.
STATUS_UNAVAILABLE - Static variable in interface jain.protocol.ss7.oam.sccp.SccpSapMBean
  A SCCP SAP Availability Status constant: Indicates that the status of the Access Point is UnAvailable.
stopPollingStatistic(Integer) - Method in interface jain.protocol.ss7.oam.OamManagedObjectMBean
  Stops the polling of statistic of the specified statistic type.

## T

TCAP_ALARM_RESOURCE_LIMIT_REACHED - Static variable in class jain.protocol.ss7.oam.tcap.TcapAlarmNotification
  Alarm Type Constant: No resources remaining.
TCAP_ERROR_DIALOGUE_ID_UNAVAILABLE - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Dialogue ID unavailable.
TCAP_ERROR_DIALOGUE_ID_UNRECOGNISED - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Unrecognised dialogue ID.
TCAP_ERROR_ILLEGAL_TIMER_EXPIRY - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Illegal timer expiry in the TCAP software.
TCAP_ERROR_INVOKE_ID_IN_USE - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Invoke ID already in use.
TCAP_ERROR_INVOKE_ID_UNRECOGNISED - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Unrecognised Involke ID.
TCAP_ERROR_MEMORY_ALLOCATION_FAILURE - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Memory allocation failure in the TCAP software.
TCAP_ERROR_MSG_MISSING_MANDATORY_PARAM - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Mandatory parameter missing.
TCAP_ERROR_MSG_UNEXPECTED_TYPE - Static variable in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Unexpected Message Type.
TCAP_PROT_ERR_COMP_PORT - Static variable in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  A TCAP Statisctic Type constant: Protocol error detected in component portion.
TCAP_PROT_ERR_TRANS_PORT1 - Static variable in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  A TCAP Statisctic Type constant: Protocol error detected in transaction portion.
TCAP_PROT_ERR_TRANS_PORT2 - Static variable in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  A TCAP Statisctic Type constant: Protocol error detected in transaction portion.
TCAP_TOTAL_RECEIVED - Static variable in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  A TCAP Statisctic Type constant: Total number of messages received by the node.
TCAP_TOTAL_SENT - Static variable in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  A TCAP Statisctic Type constant: Total number of TC messages sent by the node.
TcapAlarmNotification - class jain.protocol.ss7.oam.tcap.TcapAlarmNotification.
  A TcapAlarmNotification is a Notification emitted by a Tcap Managed Bean (MBean) to indicate a change in status of the MBean.
TcapAlarmNotification(OamManagedObjectMBean, long, int, int) - Constructor for class jain.protocol.ss7.oam.tcap.TcapAlarmNotification
  Constructs a new `TcapAlarmNotification`.
TcapErrorNotification - class jain.protocol.ss7.oam.tcap.TcapErrorNotification.
  This Notification may be emitted by any Tcap Layer Manager MBean if a user defined error is encountered.
TcapErrorNotification(OamManagedObjectMBean, long, int) - Constructor for class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Constructs a new TcapErrorNotification of the specified Error Type.
TcapLayerManagerMBean - interface jain.protocol.ss7.oam.tcap.TcapLayerManagerMBean.
  This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
TcapManagedObjectMBean - interface jain.protocol.ss7.oam.tcap.TcapManagedObjectMBean.
  This interface is used by an MBean to emit three differect types of Tcap Notifications.
TcapNodeMBean - interface jain.protocol.ss7.oam.tcap.TcapNodeMBean.
  This interface defines a local TCAP Node.
TcapStatisticNotification - class jain.protocol.ss7.oam.tcap.TcapStatisticNotification.
  An TcapStatisticNotification is a Notification emitted by an TcapManagedObjectMBean containing the value of a particular statistic.
TcapStatisticNotification(OamManagedObjectMBean, long, int, int, int) - Constructor for class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  Constructs a new `TcapStatisticNotification`.
TooManyInstancesException - exception jain.protocol.ss7.oam.TooManyInstancesException.
  This Exception is thrown whenever an attempt is made to set or create more elements than a particular implementation permits.
TooManyInstancesException(String) - Constructor for class jain.protocol.ss7.oam.TooManyInstancesException
  Constructs a new `TooManyInstancesException` identifying the OAM Managed MBean type that caused the Exception to be thrown
TooManyInstancesException(String, String) - Constructor for class jain.protocol.ss7.oam.TooManyInstancesException
  Constructs a new `TooManyInstancesException` with the specified detail message and the object Type of the managed object that caused the exception
toString() - Method in class jain.protocol.ss7.oam.mtp2.Mtp2StatisticNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.mtp2.Mtp2ErrorNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.mtp2.Mtp2AlarmNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.mtp3.Mtp3ErrorNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.mtp3.Mtp3StatisticNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.mtp3.Mtp3AlarmNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.sccp.SccpStatisticNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.sccp.SccpErrorNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.sccp.SccpAlarmNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.tcap.TcapErrorNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.tcap.TcapAlarmNotification
  Returns a string representation (with details) of classes which extend this class.
toString() - Method in class jain.protocol.ss7.oam.tcap.TcapStatisticNotification
  Returns a string representation (with details) of classes which extend this class.
TYPE_SEP - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Signalling Type constant: Indicates a Signalling End Point.
TYPE_STEP - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Signalling Type constant: Indicates a Signalling Transfer End Point.
TYPE_STP - Static variable in interface jain.protocol.ss7.oam.mtp3.SignallingPointMBean
  A Signalling Type constant: Indicates a Signalling Transfer Point.

A B C D E G H I J L M N O P R S T

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems