Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package jain.protocol.ss7.oam.mtp3

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 3 layer.

See:
Description

Interface Summary
LinkMBean | This interface defines the methods of a Link Managed Bean.
LinkSetMBean | This interface defines the methods of a Linkset to an adjacent node.
Mtp3LayerManagerMBean | This interface defines the methods required for the creation and management of all MTP Level 3 Managed MBeans.
Mtp3ManagedObjectMBean | This interface is used by an MBean to emit three differect types of Mtp3 Notifications.
Mtp3SapMBean | This interface identifies an Mtp3 Service Access Point (SAP).
Mtp3TimerProfileMBean | This interface defines the specified timers for the MTP3 Protocol Layer .
OwnSignallingPointMBean | This interface defines the methods of a Local Signalling Point Managed Bean(MBean).
RouteMBean | This interface defines the methods of a Route Managed Bean (RouteMBean).
RouteSetMBean | This interface defines the methods of a Routeset Managed Bean (RouteSetMBean).
ScreeningTableMBean | This interface defines the methods of an STP Screening Table Managed Bean(MBean).
SignallingPointMBean | This interface identifies an Signalling Point.

Class Summary
Mtp3AlarmNotification | A Mtp3AlarmNotification is a Notification emitted by a Mtp3 Managed Bean(MBean) to indicate a change in status of the MBean.
Mtp3ErrorNotification | This Notification may be emitted by any Mtp3 Managed Bean if a user defined error is encountered.
Mtp3StatisticNotification | An Mtp3StatisticNotification is a Notification emitted by an Mtp3ManagedObjectMBean containing the value of a particular statistic.

## Package jain.protocol.ss7.oam.mtp3 Description

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 3 layer. The diagram below shows the relationships between the MTP3 Managed Beans.

- The MTP3 Layer can support multiple local signalling points (OwnSignallingPointMBeans). i.e. multiple logical signalling points in the case of a loop back configuration.
- Each local signalling point can configure its own MTP3 Timers.
- The MTP3 SAP (Mtp3SapMBean) represents any signalling point. On its own, the MTP3 SAP represents a remote signalling point, and is extended by OwnSignallingPointMBean to represent a local signalling point.
- Each OwnSignallingPointMBean may have a number of ScreeningTableMBeans associated with it. The ScreeningTableMBean allows the optional SS7 functionality for an STP to identify and to handle unauthorized SS7 messages. It identifies valid destination signalling points (Mtp3SapMBeans)
- Each RouteSetMBean has a destination signalling point (Mtp3SapMBean) associated with it.
- Each LinkMBean has a single MtpSapMBean associated with it. The MTP2 SAP holds the characteristics of the physical link & port (currently only the clocking type)

Relationship between the MTP3 JAIN OAM MBeans

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems