Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package jain.protocol.ss7.oam.tcap

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the TCAP layer.

See:
Description

Interface Summary
TcapLayerManagerMBean | This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
TcapManagedObjectMBean | This interface is used by an MBean to emit three differect types of Tcap Notifications.
TcapNodeMBean | This interface defines a local TCAP Node.

Class Summary
TcapAlarmNotification | A TcapAlarmNotification is a Notification emitted by a Tcap Managed Bean (MBean) to indicate a change in status of the MBean.
TcapErrorNotification | This Notification may be emitted by any Tcap Layer Manager MBean if a user defined error is encountered.
TcapStatisticNotification | An TcapStatisticNotification is a Notification emitted by an TcapManagedObjectMBean containing the value of a particular statistic.

## Package jain.protocol.ss7.oam.tcap Description

This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the TCAP layer. The diagram below shows the relationships between the TCAP Managed Beans.

- The TcapMBean represents a local TCAP. There will be one instance of a local TCAP per local signalling point. Where multiple logical signalling points exist within the one physical stack, there will be several local TCAP instances.
- One TcapLayerManager shall manage all of the TCAP instances.

Relationship between the TCAP JAIN OAM MBeans

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems