Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Package
jain.protocol.ss7.oam

Packages that use jain.protocol.ss7.oam
jain.protocol.ss7.oam | This package contains the main interfaces and classes of the JAIN Operations, Administration and Maintenance API.
jain.protocol.ss7.oam.mtp2 | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 2 layer.
jain.protocol.ss7.oam.mtp3 | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 3 layer.
jain.protocol.ss7.oam.sccp | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the SCCP layer.
jain.protocol.ss7.oam.tcap | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the TCAP layer.

Classes in jain.protocol.ss7.oam used by jain.protocol.ss7.oam
CommitException This Exception is thrown by a JAIN OAM Managed MBean if the commit() command has been invoked and not all of the operations were successfully comitted.
IllegalOperationException This Exception is thrown if a method has been invoked that is supported by the implementation, but cannot be performed given the current state of the system.
OamLookupTable This interface provides a mechanism for an application to map between a MBean's ObjectName and a reference.
OamStatisticNotification An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
ReadConfigurationException This Exception is thrown by a JAIN OAM Layer object if the readCurrentConfiguration() method has been invoked and an error is encountered while attempting to establish the current system configuration or while creating the Managed MBeans that represent the current system configuration.
StatisticNotSupportedException This Exception is thrown if the collection of a statistic that is not supported by the underlying Stack management system has been requested.

Classes in jain.protocol.ss7.oam used by jain.protocol.ss7.oam.mtp2
OamAlarmNotification An OamAlarmNotification is a Notification emitted by a JAIN OAM Layer Manager MBean to indicate a change in status of the MBean.
OamErrorNotification This Notification may be emitted by any OAMLayerManagerMBean object if an error is encountered.
OamLayerManagerMBean This interface defines the methods common to all Protocol Layer Managers.
OamManagedObjectMBean This interface is implemented by all JAIN OAM Managed Beans (MBeans).
OamStatisticNotification An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
OamTimerProfileMBean An Oam Timer Profile is used to store all the OAM Timer Values for a particular Protocol Layer.
TooManyInstancesException This Exception is thrown whenever an attempt is made to set or create more elements than a particular implementation permits.

Classes in jain.protocol.ss7.oam used by jain.protocol.ss7.oam.mtp3
IllegalOperationException This Exception is thrown if a method has been invoked that is supported by the implementation, but cannot be performed given the current state of the system.
OamAlarmNotification An OamAlarmNotification is a Notification emitted by a JAIN OAM Layer Manager MBean to indicate a change in status of the MBean.
OamErrorNotification This Notification may be emitted by any OAMLayerManagerMBean object if an error is encountered.
OamLayerManagerMBean This interface defines the methods common to all Protocol Layer Managers.
OamManagedObjectMBean This interface is implemented by all JAIN OAM Managed Beans (MBeans).
OamStatisticNotification An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
OamTimerProfileMBean An Oam Timer Profile is used to store all the OAM Timer Values for a particular Protocol Layer.
TooManyInstancesException This Exception is thrown whenever an attempt is made to set or create more elements than a particular implementation permits.

Classes in jain.protocol.ss7.oam used by jain.protocol.ss7.oam.sccp
OamAlarmNotification An OamAlarmNotification is a Notification emitted by a JAIN OAM Layer Manager MBean to indicate a change in status of the MBean.
OamErrorNotification This Notification may be emitted by any OAMLayerManagerMBean object if an error is encountered.
OamLayerManagerMBean This interface defines the methods common to all Protocol Layer Managers.
OamManagedObjectMBean This interface is implemented by all JAIN OAM Managed Beans (MBeans).
OamStatisticNotification An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
OamTimerProfileMBean An Oam Timer Profile is used to store all the OAM Timer Values for a particular Protocol Layer.
TooManyInstancesException This Exception is thrown whenever an attempt is made to set or create more elements than a particular implementation permits.

Classes in jain.protocol.ss7.oam used by jain.protocol.ss7.oam.tcap
OamAlarmNotification An OamAlarmNotification is a Notification emitted by a JAIN OAM Layer Manager MBean to indicate a change in status of the MBean.
OamErrorNotification This Notification may be emitted by any OAMLayerManagerMBean object if an error is encountered.
OamLayerManagerMBean This interface defines the methods common to all Protocol Layer Managers.
OamManagedObjectMBean This interface is implemented by all JAIN OAM Managed Beans (MBeans).
OamStatisticNotification An OamStatisticNotification is a Notification emitted by a JAIN OAM Managed Bean(MBean) to indicate a statistic measurement of a specified MBean.
TooManyInstancesException This Exception is thrown whenever an attempt is made to set or create more elements than a particular implementation permits.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems