Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

## Uses of Interface
jain.protocol.ss7.oam.OamManagedObjectMBean

Packages that use OamManagedObjectMBean
jain.protocol.ss7.oam.mtp2 | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 2 layer.
jain.protocol.ss7.oam.mtp3 | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the MTP Level 3 layer.
jain.protocol.ss7.oam.sccp | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the SCCP layer.
jain.protocol.ss7.oam.tcap | This package contains all of the classes and interfaces that are required to provision and maintain an SS7 stack at the TCAP layer.

Uses of OamManagedObjectMBean in jain.protocol.ss7.oam.mtp2

Subinterfaces of OamManagedObjectMBean in jain.protocol.ss7.oam.mtp2
`interface` | `Mtp2LayerManagerMBean` This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
`interface` | `Mtp2ManagedObjectMBean` This interface is used by an MBean to emit three differect types of Mtp2 Notifications.
`interface` | `Mtp2SapMBean` This interface identifies an Mtp2 Service Access Point (SAP), an MTP2 SAP contains the attributes of the physical port and link that is connected to the logical signalling link.
`interface` | `Mtp2TimerProfileMBean` This interface defines the specified timers for the MTP2 Protocol Layer.

Constructors in jain.protocol.ss7.oam.mtp2 with parameters of type OamManagedObjectMBean
`Mtp2StatisticNotification.Mtp2StatisticNotification(OamManagedObjectMBean source, long sequenceNumber, int category, int statisticType, int statisticValue)` Constructs a new `Mtp2StatisticNotification`.
`Mtp2ErrorNotification.Mtp2ErrorNotification(OamManagedObjectMBean source, long sequenceNumber, int errorType)` Constructs a new Mtp2ErrorNotification of the specified Error Type.
`Mtp2AlarmNotification.Mtp2AlarmNotification(OamManagedObjectMBean source, long sequenceNumber, int priority, int alarmType)` Constructs a new `Mtp2AlarmNotification`.

Uses of OamManagedObjectMBean in jain.protocol.ss7.oam.mtp3

Subinterfaces of OamManagedObjectMBean in jain.protocol.ss7.oam.mtp3
`interface` | `LinkMBean` This interface defines the methods of a Link Managed Bean.
`interface` | `LinkSetMBean` This interface defines the methods of a Linkset to an adjacent node.
`interface` | `Mtp3LayerManagerMBean` This interface defines the methods required for the creation and management of all MTP Level 3 Managed MBeans.
`interface` | `Mtp3ManagedObjectMBean` This interface is used by an MBean to emit three differect types of Mtp3 Notifications.
`interface` | `Mtp3SapMBean` This interface identifies an Mtp3 Service Access Point (SAP).
`interface` | `Mtp3TimerProfileMBean` This interface defines the specified timers for the MTP3 Protocol Layer .
`interface` | `OwnSignallingPointMBean` This interface defines the methods of a Local Signalling Point Managed Bean(MBean).
`interface` | `RouteMBean` This interface defines the methods of a Route Managed Bean (RouteMBean).
`interface` | `RouteSetMBean` This interface defines the methods of a Routeset Managed Bean (RouteSetMBean).
`interface` | `ScreeningTableMBean` This interface defines the methods of an STP Screening Table Managed Bean(MBean).
`interface` | `SignallingPointMBean` This interface identifies an Signalling Point.

Constructors in jain.protocol.ss7.oam.mtp3 with parameters of type OamManagedObjectMBean
`Mtp3ErrorNotification.Mtp3ErrorNotification(OamManagedObjectMBean source, long sequenceNumber, int errorType)` Constructs a new Mtp3ErrorNotification of the specified Error Type.
`Mtp3StatisticNotification.Mtp3StatisticNotification(OamManagedObjectMBean source, long sequenceNumber, int category, int statisticType, int statisticValue)` Constructs a new `Mtp3StatisticNotification`.
`Mtp3AlarmNotification.Mtp3AlarmNotification(OamManagedObjectMBean source, long sequenceNumber, int priority, int alarmType)` Constructs a new `Mtp3AlarmNotification`.

Uses of OamManagedObjectMBean in jain.protocol.ss7.oam.sccp

Subinterfaces of OamManagedObjectMBean in jain.protocol.ss7.oam.sccp
`interface` | `ConcernedAreaMBean` This interface contains a list of remote Subsystems (SccpSaps) to be informed of local (primary broadcast) or remote (secondary broadcast) SCCP Subsystem status changes, or to be informed of the SCCP status after completion of SCCP Restart.
`interface` | `GlobalTitleEntryMBean` This class represents a Global Title entry (a combination of the global title translator and global title rule).
`interface` | `SccpEntitySetMBean` This class identifies the set of access points that result from a global title translation.
`interface` | `SccpLayerManagerMBean` This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
`interface` | `SccpManagedObjectMBean` This interface is used by an MBean to emit three differect types of Sccp Notifications.
`interface` | `SccpRoutingControlMBean` This interface defines the methods required by the SCCP Routing Control Function It defines methods to maintain management information concerning the SCCP routing control.
`interface` | `SccpSapMBean` This interface defines a SCCP Access Point (an SCCP Subsystem).
`interface` | `SccpTimerProfileMBean` This interface defines the specified timers for the SCCP Protocol Layer.

Constructors in jain.protocol.ss7.oam.sccp with parameters of type OamManagedObjectMBean
`SccpStatisticNotification.SccpStatisticNotification(OamManagedObjectMBean source, long sequenceNumber, int category, int statisticType, int statisticValue)` Constructs a new `SccpStatisticNotification`.
`SccpErrorNotification.SccpErrorNotification(OamManagedObjectMBean source, long sequenceNumber, int errorType)` Constructs a new SccpErrorNotification of the specified Error Type.
`SccpAlarmNotification.SccpAlarmNotification(OamManagedObjectMBean source, long sequenceNumber, int priority, int alarmType)` Constructs a new `SccpAlarmNotification`.

Uses of OamManagedObjectMBean in jain.protocol.ss7.oam.tcap

Subinterfaces of OamManagedObjectMBean in jain.protocol.ss7.oam.tcap
`interface` | `TcapLayerManagerMBean` This interface defines the methods required for the creation and management of all MTP Level 2 Managed MBeans.
`interface` | `TcapManagedObjectMBean` This interface is used by an MBean to emit three differect types of Tcap Notifications.
`interface` | `TcapNodeMBean` This interface defines a local TCAP Node.

Constructors in jain.protocol.ss7.oam.tcap with parameters of type OamManagedObjectMBean
`TcapErrorNotification.TcapErrorNotification(OamManagedObjectMBean source, long sequenceNumber, int errorType)` Constructs a new TcapErrorNotification of the specified Error Type.
`TcapAlarmNotification.TcapAlarmNotification(OamManagedObjectMBean source, long sequenceNumber, int priority, int alarmType)` Constructs a new `TcapAlarmNotification`.
`TcapStatisticNotification.TcapStatisticNotification(OamManagedObjectMBean source, long sequenceNumber, int category, int statisticType, int statisticValue)` Constructs a new `TcapStatisticNotification`.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

11 August 2000

Copyright - 2000 Sun Microsystems